CC1902RL Underway Data Processing Notes

The raw UW data were extracted from the various files in the UW Directory structure.

**Notes:**

TSG-SBE45 did not function or was not online.

No meaningful underway fluorometer data are available.

**The available variables from these files are:**

DateTime, Date, Time – these are UTC

COG – course over ground (deg)

SOG – ship speed over ground (knots)

USWFlow – seawater flow rate (Flowmeter-Bow) (gal/min ?)

LongWaveRad – Long Wave Radiation (W/M2, Pyranometer)

ShortWaveRad - Short Wave Radiation (W/M2, Pyranometer)

WindSpeed – wind speed (m/sec)

WindDir – wind direction (deg)

AirTemp – air temperature (deg C)

AtmPress – atmospheric pressure (mb)

RelHum – relative humidity (% saturation)

TSG\_Temp – temperature measured by the Reuben Lasker TSG SBE 21 unit (deg C)

TSG\_Cond – conductivity measured by the Reuben Lasker TSG SBE 21 unit (mSi/m2)

TSG\_Sal – salinity calculated by the Reuben Lasker TSG SBE 21 unit (PSU)

TSG\_Dens – density calculated by the ship’s systems from Temp and Cond

SoundVel – sound velocity (m/sec)

SSTemp – sea surface temperature from unknown sensor (deg C)

ChlFluor – chlorophyll fluorescence (volt); No meaningful underway fluorometer data are available

**Derived variables are:**

Pred\_Temp – temperature derived from calibrations of TSG\_Temp vs. CalCOFI 0 to 12 m bottle temperatures (deg C)

Pred\_Sal – salinity derived from calibrations of TSG\_Sal vs. CalCOFI 0 to 12 m bottle salinity (PSU)