CC1907BH Underway Data Processing Notes

The R/V Bold Horizon did not have an operating TSG system. The data below are from the ship’s meteorological sensors and the Todd Martz Lab’s pCO2/pH system. Thus a variety of variables were not measured.

There must have been problems with the UW system water flow rates since the CalCOFI bottle 0 to 10 m temp differed significantly from the UW temp measurements. The two Sal measurements compared well.

**The available UW variables from CC1907BH are:**

COG – course over ground (deg)

SOG – ship speed over ground (knots)

(USWFlow – not available) – measure of water flow through the UW system (varying units)

(PARSurf – not available) – photosynthetically available radiation measured aboard the ship (uE/Sec/Meter2)

(LongWaveRad – not available) – Long Wave Radiation (W/M2, Pyranometer)

(ShortWaveRad – not available) – Short Wave Radiation (W/M2, Pyranometer)

WindSpeed – wind speed (m/sec)

WindDir – wind direction (deg)

AirTemp – air temperature (deg C)

AtmPress – atmospheric pressure (mb)

RelHum – relative humidity (% saturation)

TSG\_Temp – water temperature measured by the STBD-TSG-Flowthrough unit (deg C)

(TSG\_Temp2 – not available) – water temperature (deg C)

TSG\_Cond – water conductivity measured by the STBD-TSG-Flowthrough unit (mS/cm)

TSG\_Sal – water salinity calculated by the STBD-TSG-Flowthrough unit (PSU)

TSG\_Dens – water density as sigma-t calculated by the STBD-TSG-Flowthrough unit (PSU)

SoundVel – sound velocity calculated by the Sally Ride’s TSG75 unit (m/sec)

(TSG\_Temp\_2 – not available) – water temperature (deg C)

(TSG\_Cond\_2 – not available) – water conductivity (mS/cm)

(TSG\_Sal\_2 – not available) – water salinity calculated (PSU)

(TSG\_Dens\_2 – not available) – water density as sigma-t (PSU)

(SoundVel\_2 – not available) – sound velocity (m/sec)

(Oxygen – not available) – oxygen concentrations (mL/L)

(OxygenSat – not available) – oxygen saturation (%)

(SSTemp - Sea Surface Temperature, SBE 48 hull mount (degC)

(ChlFluor – chlorophyll fluorescence (volt) – The instrument must have malfunctioned. No meaningful correlation between ChlFluor and CalCOFI bottle Chl values was observed.


**Derived variables are:**

Pred\_Temp – temperature derived from calibrations of TSG\_Temp vs. CalCOFI 0 to 12 m bottle temperatures (deg C)


Pred\_Sal – salinity derived from calibrations of TSG\_Sal vs. CalCOFI 0 to 12 m bottle salinity (PSU)

(Pred\_Chl – chlorophyll derived from calibrations of ChlFluor vs. CalCOFI 0 to 12 m bottle Chl a (ug-Chl/L). All values are set to NaN.

Temperature Calibration: Todd Martz TSG\_Temp vs. CalCOFI Bottle  
There are some problems with water heating in the UW pipe system likely caused by UW flow instability.



Salinity Calibration: Todd Martz TSG\_Sal vs. CalCOFI Bottle



Chl-a Calibration: R/Vx Flouro vs. CalCOFI Bottle  
(no data available for this cruise)