****Event Report File - SCS 4.0****

Event Header File - TsgTransmitter_001.hdr
Event started on 1/11/2013 at 5:34:02 PM

Ship Meta Data
    HDR_WMOID:WTED
    HDR_SHIPN:NOAA Ship Bell M Shimada
    HDR_TECM:ChiefET.bell.shimada@noaa.gov
    HDR_TECAM:chiefst.bell.shimada@noaa.gov

TSG Meta Data
    HDR_IMONO:9349069
    HDR_TSGMOD:SBE-21
    HDR_TSGSN:3318
    HDR_IDP:4.9 m
    HDR_ILEN:30 m
    HDR_DCAL:13-Nov-12

TSG Cal Constants
    HDR_COTG:4.16272586e-003
    HDR_COTH:6.13406029e-004
    HDR_COTI:1.84346406e-005
    HDR_COTJ:1.30382720e-006
    HDR_COTF0:1000
    HDR_COCG:-3.99580677e+000
    HDR_COCH:4.72891290e-001
    HDR_COCI:-5.76434811e-004
    HDR_COCJ:5.27566093e-005
    HDR_COCPR:-9.5700e-008
    HDR_COCTR:3.2500e-006

SBE38 Metadata
    HDR_COA0:6.050766e-005
    HDR_COA1:2.738465e-004
    HDR_COA2:-2.411317e-006
    HDR_COA3:1.522687e-007
    HDR_COSL:0.00
    HDR_COTO:0.00
    HDR_EXTMOD:SBE-38
    HDR_EXTSN:0701
    HDR_EXTTD:4.9M
    HDR_EXTDCAL:09-Dec-12

Sea Surface Temp Metadata
    HDR_SSTMOD:SBE-38
    HDR_SSTSN:0701
    HDR_SSTD:4.9M
    HDR_SSTDCAL:09-Dec-12

Sensor Designators
    LAT:3237.1563N
    LON:11715.5106W
    INT:22.37639
    SAL:33.70865
    COND: 3.85235
    SST:11.63230

Output: TSG-OBS ; Type: File
    Output Mode: Continuous every 30 second(s)
    Fields in output record:
        Date
        Time
        SciGPS-Lat (DDMM.MM)
        SciGPS-Lon (DDMM.MM)
        TSG21-InternalTemp-C (deg C)
        TSG21-SeaSurfaceSalinity-PPT (PSU)
        TSG21-SeaSurfaceConductivity (S/m)
        TSG21-SBE38-SeaSurfaceTemp-C (deg C)

Event stopped at 2/2/2013 at 5:05:15 PM

********End of Report File********
