****Event Report File - SCS 4.0****

Event Header File - NODC_001.hdr
Event started on 1/11/2013 at 5:40:32 PM

NODC
    SHIP:Bell M. Shimada
    CAPTAIN:CDR Scott Sirois
    CRUISE:SH-12-05 Leg 1
    CHIEF SCIENTIST:Richard Feely
    SCS ADMINISTRATOR:ST Gunter
    CRUISE START DATE:04Sep2012
    CRUISE END DATE:18Sep2012

SENSOR-ID1
    PRIMARY GPS MODEL:MX420
    PRIMARY GPS MANUFACTURER:Magnavox
    PRIMARY GPS CAL DATE:Jan 2011
    SECONDARY GPS MODEL:Trimble
    SECONDARY GPS MANUFACTURER:POSMV
    SECONDARY GPS CAL DATE:Jan 2011
    DEPTH MODEL:EK60
    DEPTH MANUFACTURER:Simrad
    DEPTH CAL DATE:03-21-2011
    GYRO MODEL:Navigat X Mk1 4914-CA
    GYRO MANUFACTURER:Sperry Marine
    GYRO CAL DATE:TBD
    TSG MODEL:SBE21
    TSG MANUFACTURER:SEA-BIRD
    TSG CAL DATE:11/29/2011

SENSOR-ID2
    WIND MODEL:WM05106
    WIND MANUFACTURER:RMYoung
    WIND CAL DATE:02-10-2009
    BAROMETER MODEL:61302V
    BAROMETER MANUFACTURER:RMYOUNG
    BAROMETER CAL DATE:11-15-2011
    AIR TEMP MODEL:41382VC
    AIR TEMP MANUFACTURER:RMYOUNG
    AIR TEMP CAL DATE:2/14/2011
    HUMIDITY MODEL:41382VC
    HUMIDITY MANUFACTURER:RMYOUNG
    HUMIDITY CAL DATE:2/14/2011

Output: NODC-NAV1 ; Type: File
    Output Mode: Continuous every 30 second(s)
    Fields in output record:
        Date
        Time
        SciGPS-Time (GMT)
        SciGPS-Lat (DDMM.MM)
        SciGPS-Lon (DDMM.MM)
        SciGPS-Quality (1=std)
        SciGPS-Sats ()
        SciGPS-Hdops ()
        SciGPS-COG (deg)
        SciGPS-SOG (Knots)
        Gyro-MainFeed-Heading (deg)

Output: NODC-NAV2 ; Type: File
    Output Mode: Continuous every 30 second(s)
    Fields in output record:
        Date
        Time
        POSMV-INGGA-Time (hhmmss)
        POSMV-INGGA-Lat (DDMM.MM)
        POSMV-INGGA-Lon (DDMM.MM)
        POSMV-INGGA-Quality (1=std)
        POSMV-INGGA-Sats (NONE)
        POSMV-INGGA-hdops (NONE)
        POSMV-INVTG-COG (Degrees)
        POSMV-INVTG-SOG (Knots)
        POSMV-PASHR-Heading-True (deg)

Output: NODC-OBS ; Type: File
    Output Mode: Continuous every 30 second(s)
    Fields in output record:
        Date
        Time
        SciGPS-Time (GMT)
        SciGPS-Lat (DDMM.MM)
        SciGPS-Lon (DDMM.MM)
        POSMV-INGGA-Lon (DDMM.MM)
        POSMV-INGGA-Lat (DDMM.MM)
        POSMV-INGGA-Time (hhmmss)
        TSG21-SBE38-SeaSurfaceTemp-C (deg C)
        TSG21-SeaSurfaceSalinity-PPT (PSU)
        TSG21-SeaSurfaceConductivity (S/m)
        AirTempC (Deg-c)
        RelativeHumidity (PERCENT)
        TrueWind-FwdJackStaff-Speed (Deg/Knots)
        TrueWind-FwdJackStaff-Direction (Deg/Knots)
        RelativeWindSpeed-kts-FwdJackStaff (Knots)
        RelativeWindDirection-FwdJackStaff (deg)
        BarometricPressureTrue-mBars-Value (mBars)

Event stopped at 1/11/2013 at 5:55:18 PM

********End of Report File********
