\documentclass[12pt]{article}
\title{BGM3 tilt test report}
\author{Maxwell Hughes, vessel: R/V Sally Ride}
\date{Release Date: 2022/02/25 21:57:43 UTC}
\begin{document}
\maketitle
Sensor: S224

Software version: 1.2

Port/Pier/Berth: MarFac

\begin{table}[h]
\centering
\begin{tabular}{ | c | c | }
\hline
Axis & roll\\ \hline 
Filtered gravity 1 & 979532.18\\ \hline 
Filtered gravity 2 & 979535.41\\ \hline 
Misalignment & -1.1623122 mrad \\ \hline 
Tolerance & 0.7mrad \\ \hline \hline
\end{tabular}
\caption{Gravity readings and misalignment}
\end{table}

Action: Turn potentiometer R41 on Gyro Electronics CPS board 4.6 turns in CW direction, then retest.

\end{document}

