\documentclass[12pt]{article}
\title{BGM3 tilt test report}
\author{Howell Johnson, Maxwell Hughes, vessel: R/V Sally Ride}
\date{Release Date: 2022/05/17 21:25:30 UTC}
\begin{document}
\maketitle
Sensor: S224

Software version: 1.2

Port/Pier/Berth: MarFac

\begin{table}[h]
\centering
\begin{tabular}{ | c | c | }
\hline
Axis & roll\\ \hline 
Filtered gravity 1 & 979532.77\\ \hline 
Filtered gravity 2 & 979537.26\\ \hline 
Misalignment & -1.6188067 mrad \\ \hline 
Tolerance & 0.7mrad \\ \hline \hline
\end{tabular}
\caption{Gravity readings and misalignment}
\end{table}

Action: Turn potentiometer R41 on Gyro Electronics CPS board 6.5 turns in CW direction, then retest.

\end{document}

